#!/bin/sh

printf "Hold down the HackRF's DFU button (the button closest to the antenna jack)\n"
printf "then plug the HackRF into a USB port on your computer.\n\n"
printf "After the HackRF is plugged in, you may release the DFU button.\n"
printf "Press any key to continue or ^c to abort\n"
read

dfu-util --device 1fc9:000c --download hackrf_one_usb_ram.dfu --reset
sleep 2s
hackrf_spiflash -w portapack-h1-firmware.bin
